Dismantling and removing of damaged/burnt power and control cables of phase-2 crusher house and laying and fixing with help of clamps new power and control cables which will be provided departmentally

Lubrication panel

Crusher control panel

Hydraulic panel

Dust suppression system control panel

Heat exchanger control panel

Dust extraction system control panel

Ventilation system control panel

Power distribution panel

--

Supply of straight through jointing kit suitable for 3 x 50 sq mm, 11kV grade armoured HT cable - 1no

--

Supply of straight through cable suitable for 4x240sq mm 1.1 kV grade armoured LT cable – 4no

--

Supply of straight though cable suitable for 4 x 95 sq mm 1.1 kV grade armoured LT cable -4 no

--

Supply of straight though cable suitable for 4 x 50 sq mm 1.1 kV grade armoured LT cable -6 no

--

Replacement of cable by removing damaged portion of the cable and laying of new PVC armoured copper cable 4 x 50 sq. mm, 60m length along the cable trays of crusher house and jointing the cable with existing cables with 11kV grade HT cable jointing kit. The cable will be provided departmentally however jointing kit will supplied by the contractor.