|  |  |  |
| --- | --- | --- |
| Sub | : | Indent for procurement of level sensor for silo |
| Indent Amount | : | Rs. |
| Please find enclosed herewith an indent Indent for procurement of level sensor for silo.  These level sensors are required for smooth running of the CHP. Level sensor display the level upto which coal in filled in silo. Also it prevents overfilling of the silo, which may cause spillage.  Exiting level sensors are of ultrasonic type, which have poor accuracy for bulk solid type of material like coal. However, newer and better technology like radar type sensors are now readily available in market, which do not have the shortcomings of ultrasonic sensors, therefore have better accuracy.  This item is not available in GEM portal.  This item is not included in MSME reserved list.  The item is decentralized spare in nature.  Put up for kind approval.    Encl: INDT/20-21/1037/ dtd. | | |
| In-charge, CHP  Dudhichua Project | | |