To

Area safety officer,

Dudhichua area.

**Sub: Compliance of observations of safety committee for inspection on dated 29-10-2020.**

Pt-1: The heap of coal at receiving pit of crushers are caused by dozers/payloaders while pushing coal into the receiving pit. This is not a CHP housekeeping issue. To mitigate this problem, the practice of dozing coal into the receiving pit must be stopped.

Pt-2: Fencing of conveyor walkways, wherever required has been done.

Pt-3: Civil department has been communicated with this matter. Drainage will be cleared at the earliest.

Pt-4: Earth leakage relays are operational now. Broken lightening arrestor earthing strip has been fixed.

Pt-5: Regarding coal head over phase-2 tunnel, dispatch in-charge has been informed multiple times. Coal under conveyors are being lifted up. Dust suppression system has been rectified.

Yours faithfully

In-charge, CHP

Dudhichua Project

Copy: for kind information please.

1. GM(E&M), Dudhichua area
2. PE(E&M), Dudhichua project