***SUB: Requirement of electrical maintenance workshop facility at CHP, DCH.***

*It has been felt that for regular nature of electric maintenance works of HT & LT motors, transformers, breakers, etc. a workshop facility is indispensably required at CHP premise.*

*Following facilities and attributes are desirable in the workshop in terms of civil construction.*

* *Floor area 20m x 10m.*
* *Height 5m*
* *Monorail of capacity 10Te.*
* *Cable trench for powering from SS-5.*
* *Provision for installation of ventilation fans.*
* *Concrete flooring outside main gate for vehicle movement.*
* *Metal gate with central locking arrangement.*
* *Provision for installation of ceiling mounted lights and fans.*

*A suitable location near SS-5 has been identified for the purpose. GM (E&M), Dudhichua Project is requested to take up the matter with competent authority for approval of the proposal and further action please.*

*Yours’s faithfully*

*I/c, CHP*

*Dudhichua Project*

*PE(E&M)/Dudhichua Project*

*GM (E&M), Dudhichua Area*